F183I

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Board ID | Doc Version | Date | Author | ASIC ID | Production |
| F183I | 0.1 | 23.03.2022 | L. Ghislotti | 183 | Italian |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | **#** | **Test Description** | **Pass** | **Note** | |
| Visual | 1 | Visual inspection | Yes | See notes (if any) | |
| Bias | 2 | Analog | Yes | AVDD [V] | 1.795 |
| Yes | IVDD [mA] | 134.6 |
| Digital | Yes | DVDD [V] | 1.796 |
| Yes | IDVDD [mA] | 5 |
| Calibration | Yes | 3V3 [V] | 2.991 |
| Yes | I3V3 [mA] | 3 |
| Bias current | Yes | Ibias [mA] | 4.97 |
| Reference Voltages | Yes | VCMSH [V] | 1.197 |
| Yes | VCM [V] | 0.890 |
| Yes | RVCM [V] | 0.897 |
| Digital | 3 | Configuration test | Yes |  | |
| Wrong address test | Yes |  | |
| Temperature Sensor | Yes | ADC | 1040 |
| T [°C] | 25.947 |
| Analog | 4 | Input-output characteristic | Yes | # of non resp. ch | 0 |
| 5 | Noise ENC FWHM @ tp=6 | Yes | Ch 0 [keV] | 19.194 |
| Ch 7 [keV] | 112.494 |
| Ch 15 [keV] | 26.947 |
| Ch 16 [keV] | 23.927 |
| Ch 23 [keV] | 111.065 |
| Ch 31 [keV] | 21.425 |
| 6 | Threshold dispersion @ tp=6 | Yes | Before FT [DAC] | 5.687 |
| After FT [DAC] | 3.216 |
| 7 | Pedestal dispersion @ tp=6 | Yes | Dispersion [ADC] | 28.349 |

**Notes:**

scratches on bottom  
exposed copper on bottom